Source: dump1090-fa
Section: embedded
Priority: extra
Maintainer: Oliver Jowett <oliver@mutability.co.uk>
Build-Depends: debhelper(>=9), librtlsdr-dev, libusb-1.0-0-dev, pkg-config, dh-systemd, libncurses5-dev, libbladerf-dev
Standards-Version: 3.9.3
Homepage: http://www.flightaware.com/
Vcs-Git: https://github.com/flightaware/dump1090.git

Package: dump1090
Architecture: all
Depends: dump1090-fa, ${misc:Depends}
Priority: extra
Section: oldlibs
Description: transitional dummy package for dump1090
  This is a transitional dummy package to handle upgrades from
  the old package name of "dump1090" to the new package name of
  "dump1090-fa". It can safely be removed.

Package: dump1090-fa
Architecture: any
Depends: ${shlibs:Depends}, ${misc:Depends}, libbladerf1 (>= 0.2016.06), adduser, lighttpd
Replaces: dump1090 (<< 3.0)
Breaks: dump1090 (<< 3.0)
Description: ADS-B Ground Station System for RTL-SDR
 Networked Aviation Mode S / ADS-B decoder/translator with RTL-SDR software
 defined radio USB device support.
 .
 This is FlightAware's fork of dump1090-mutability, customized for use
 in the PiAware sdcard images.
